,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Nominal Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,Total Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,Fan Type##other##,Heating Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,Maximum Heating Input (MBH)##number##general,Maximum Heating Output (MBH)##number##general,Minimum Heating Input (MBH)##number##general,Minimum Heating Output (MBH)##number##general,System Performance EER##other##,System Performance IEER##other##,COP At 17F##other##,COP At 47F##other##,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Gas Connection Size##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Model Number##other##,Refrigerant Used##other##,Standards##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_Standard_Heat_230V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage",208 VAC - 230 VAC,240,130000,105000,85000,105000,10.9,15,2.1,3.35,620,60,3,1,0.75,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT152H5ES1Y,R-454B,ASHRAE 90.1 Compliant,5250,1750
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_Medium_Heat_230V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage",208 VAC - 230 VAC,240,180000,146000,117000,146000,10.9,15,2.1,3.35,620,60,3,1,0.75,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT152H5EM1Y,R-454B,ASHRAE 90.1 Compliant,5250,1750
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_High_Heat_230V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage",208 VAC - 230 VAC,240,240000,194000,156000,194000,10.9,15,2.1,3.35,620,60,3,1,0.75,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT152H5EH1Y,R-454B,ASHRAE 90.1 Compliant,5250,1750
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_Standard_Heat_460V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage",460 VAC,480,130000,105000,85000,105000,10.9,15,2.1,3.35,620,60,3,1,0.75,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT152H5ES1G,R-454B,ASHRAE 90.1 Compliant,5250,1750
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_Medium_Heat_460V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage",460 VAC,480,180000,146000,117000,146000,10.9,15,2.1,3.35,620,60,3,1,0.75,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT152H5EM1G,R-454B,ASHRAE 90.1 Compliant,5250,1750
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_High_Heat_460V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage",460 VAC,480,240000,194000,156000,194000,10.9,15,2.1,3.35,620,60,3,1,0.75,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT152H5EH1G,R-454B,ASHRAE 90.1 Compliant,5250,1750
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_Standard_Heat_575V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage",575 VAC,600,130000,105000,85000,105000,10.9,15,2.1,3.35,620,60,3,1,0.75,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT152H5ES1J,R-454B,ASHRAE 90.1 Compliant,5250,1750
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_Medium_Heat_575V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage",575 VAC,600,180000,146000,117000,146000,10.9,15,2.1,3.35,620,60,3,1,0.75,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT152H5EM1J,R-454B,ASHRAE 90.1 Compliant,5250,1750
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_High_Heat_575V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage",575 VAC,600,240000,194000,156000,194000,10.9,15,2.1,3.35,620,60,3,1,0.75,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT152H5EH1J,R-454B,ASHRAE 90.1 Compliant,5250,1750
