,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Nominal Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,Total Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,Fan Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,System Performance EER##other##,System Performance IEER##other##,COP At 17F##other##,COP At 47F##other##,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Refrigerant Used##other##,Standards##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Base Rail Height##length##inches,Bottom Drain Connection Vertical Offset##length##inches,Evaporator Side Service Clearance##length##inches,Front Side Service Clearance##length##inches,Minimum Operation Clearance##length##inches,Service Clearance##length##inches,Downflow Return Duct Vertical Offset##length##inches,Downflow Supply Duct Vertical Offset##length##inches,Downflow Return Air Connection Height##hvac_duct_size##inches,Downflow Return Air Connection Width##hvac_duct_size##inches,Downflow Return Duct Horizontal Offset##length##inches,Downflow Supply Air Connection Height##hvac_duct_size##inches,Downflow Supply Air Connection Width##hvac_duct_size##inches,Downflow Supply Duct Horizontal Offset##length##inches,Drain Connection Horizontal Offset##length##inches,Drain Connection Vertical Offset##length##inches,Enclosure Depth##length##inches,Enclosure Width##length##inches,Horizontal Return Air Connection Height##hvac_duct_size##inches,Horizontal Return Air Connection Width##hvac_duct_size##inches,Horizontal Return Duct Horizontal Offset##length##inches,Horizontal Return Duct Vertical Offset##length##inches,Horizontal Supply Air Connection Height##hvac_duct_size##inches,Horizontal Supply Air Connection Width##hvac_duct_size##inches,Horizontal Supply Duct Horizontal Offset##length##inches,Horizontal Supply Duct Vertical Offset##length##inches,Outdoor Fan Diameter##length##inches
6.5Ton_High_Efficiency_Single-Zone_VAV_Blower_230V,79000,6.5,40000,73000,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,12.7,17,2.25,3.5,561,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
7.5Ton_High_Efficiency_Single-Zone_VAV_Blower_230V,92000,7.5,46000,86000,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,12.3,16.8,2.25,3.5,569,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
8.5Ton_High_Efficiency_Single-Zone_VAV_Blower_230V,101000,8.5,53000,96000,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,12.1,16.8,2.25,3.5,570,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
10Ton_High_Efficiency_Single-Zone_VAV_Blower_230V,119900,10,63000,112000,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,12.7,17,2.25,3.5,570,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
6.5Ton_High_Efficiency_Single-Zone_VAV_Blower_460V,79000,6.5,40000,73000,Single-Zone Variable Air Volume,460 VAC,480,12.7,17,2.25,3.5,561,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
7.5Ton_High_Efficiency_Single-Zone_VAV_Blower_460V,92000,7.5,46000,86000,Single-Zone Variable Air Volume,460 VAC,480,12.3,16.8,2.25,3.5,569,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
8.5Ton_High_Efficiency_Single-Zone_VAV_Blower_460V,101000,8.5,53000,96000,Single-Zone Variable Air Volume,460 VAC,480,12.1,16.8,2.25,3.5,570,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
10Ton_High_Efficiency_Single-Zone_VAV_Blower_460V,119900,10,63000,112000,Single-Zone Variable Air Volume,460 VAC,480,12.7,17,2.25,3.5,570,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
6.5Ton_High_Efficiency_Single-Zone_VAV_Blower_575V,79000,6.5,40000,73000,Single-Zone Variable Air Volume,575 VAC,600,12.7,17,2.25,3.5,561,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
7.5Ton_High_Efficiency_Single-Zone_VAV_Blower_575V,92000,7.5,46000,86000,Single-Zone Variable Air Volume,575 VAC,600,12.3,16.8,2.25,3.5,569,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
8.5Ton_High_Efficiency_Single-Zone_VAV_Blower_575V,101000,8.5,53000,96000,Single-Zone Variable Air Volume,575 VAC,600,12.1,16.8,2.25,3.5,570,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
10Ton_High_Efficiency_Single-Zone_VAV_Blower_575V,119900,10,63000,112000,Single-Zone Variable Air Volume,575 VAC,600,12.7,17,2.25,3.5,570,60,3,1,60.125,46.875,101.25,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5250,1750,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
