,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Fan Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,System Performance EER##other##,System Performance IEER##other##,System Performance COP##other##,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Refrigerant Used##other##,Standards##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Service Clearance##length##inches,Minimum Operation Clearance##length##inches,Front Side Service Clearance##length##inches,Front Side Minimum Operation Clearance##length##inches,Evaporator Side Service Clearance##length##inches,Evaporator Side Minimum Operation Clearance##length##inches,Base Rail Height##length##inches,Bottom Drain Connection Horizontal Offset##length##inches,Bottom Drain Connection Vertical Offset##length##inches,Downflow Return Air Connection Height##hvac_duct_size##inches,Downflow Return Air Connection Width##hvac_duct_size##inches,Downflow Return Duct Horizontal Offset##length##inches,Downflow Return Duct Vertical Offset##length##inches,Downflow Supply Air Connection Height##hvac_duct_size##inches,Downflow Supply Air Connection Width##hvac_duct_size##inches,Downflow Supply Duct Horizontal Center Offset##length##inches,Downflow Supply Duct Horizontal Offset##length##inches,Downflow Supply Duct Vertical Offset##length##inches,Horizontal Return Air Connection Height##hvac_duct_size##inches,Horizontal Return Air Connection Width##hvac_duct_size##inches,Horizontal Return Duct Horizontal Offset##length##inches,Horizontal Return Duct Vertical Offset##length##inches,Horizontal Roof Curb Depth##length##inches,Horizontal Roof Curb Width##length##inches,Horizontal Supply Air Connection Width##hvac_duct_size##inches,Outdoor Fan Diameter##length##inches,Side Drain Connection Horizontal Offset##length##inches,Side Drain Connection Vertical Offset##length##inches,Unit Base Width##length##inches
15Ton_MSAV_Blower_Standard_Efficiency_230V,176000,15,MSAV Multi-Stage Air Volume,208 VAC - 230 VAC,240,10.6,13.5,3.3,2374,60,3,1,91.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,R-454B,ASHRAE 90.1 Compliant,11000,3250,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75
20Ton_MSAV_Blower_Standard_Efficiency_230V,224000,20,MSAV Multi-Stage Air Volume,208 VAC - 230 VAC,240,10.6,13.5,3.3,2411,60,3,1,91.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,R-454B,ASHRAE 90.1 Compliant,11000,3250,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75
15Ton_MSAV_Blower_Standard_Efficiency_460V,176000,15,MSAV Multi-Stage Air Volume,460 VAC,480,10.6,13.5,3.3,2374,60,3,1,91.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,R-454B,ASHRAE 90.1 Compliant,11000,3250,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75
20Ton_MSAV_Blower_Standard_Efficiency_460V,224000,20,MSAV Multi-Stage Air Volume,460 VAC,480,10.6,13.5,3.3,2411,60,3,1,91.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,R-454B,ASHRAE 90.1 Compliant,11000,3250,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75
15Ton_MSAV_Blower_Standard_Efficiency_600V,176000,15,MSAV Multi-Stage Air Volume,575 VAC,600,10.6,13.5,3.3,2374,60,3,1,91.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,R-454B,ASHRAE 90.1 Compliant,11000,3250,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75
20Ton_MSAV_Blower_Standard_Efficiency_600V,224000,20,MSAV Multi-Stage Air Volume,575 VAC,600,10.6,13.5,3.3,2411,60,3,1,91.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,R-454B,ASHRAE 90.1 Compliant,11000,3250,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75
