,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Fan Type##other##,Heating Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,Maximum Heating Input (MBH)##number##general,Maximum Heating Output (MBH)##number##general,Minimum Heating Input (MBH)##number##general,Minimum Heating Output (MBH)##number##general,Maximum Overcurrent Protection##electrical_current##amperes,Minimum Circuit Amps##electrical_current##amperes,System Performance EER##other##,System Performance IEER##other##,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Gas Connection Size##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Model Number##other##,Refrigerant Used##other##,Standards##other##,Service Clearance##length##inches,Clearance to Combustibles##length##inches,Minimum Operation Clearance##length##inches,Front Side Service Clearance##length##inches,Front Side Clearance to Combustibles##length##inches,Front Side Minimum Operation Clearance##length##inches,Evaporator Side Service Clearance##length##inches,Evaporator Side Minimum Operation Clearance##length##inches,Base Rail Height##length##inches,Bottom Drain Connection Horizontal Offset##length##inches,Bottom Drain Connection Vertical Offset##length##inches,Bottom Gas Connection Vertical Offset##length##inches,Downflow Return Air Connection Height##hvac_duct_size##inches,Downflow Return Air Connection Width##hvac_duct_size##inches,Downflow Return Duct Horizontal Offset##length##inches,Downflow Return Duct Vertical Offset##length##inches,Downflow Supply Air Connection Height##hvac_duct_size##inches,Downflow Supply Air Connection Width##hvac_duct_size##inches,Downflow Supply Duct Horizontal Center Offset##length##inches,Downflow Supply Duct Horizontal Offset##length##inches,Downflow Supply Duct Vertical Offset##length##inches,Gas Connection Horizontal Offset##length##inches,Horizontal Return Air Connection Height##hvac_duct_size##inches,Horizontal Return Air Connection Width##hvac_duct_size##inches,Horizontal Return Duct Horizontal Offset##length##inches,Horizontal Return Duct Vertical Offset##length##inches,Horizontal Roof Curb Depth##length##inches,Horizontal Roof Curb Width##length##inches,Horizontal Supply Air Connection Width##hvac_duct_size##inches,Outdoor Fan Diameter##length##inches,Side Drain Connection Horizontal Offset##length##inches,Side Drain Connection Vertical Offset##length##inches,Top Gas Connection Vertical Offset##length##inches
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Low_Heat_230V,148000,13,Single-Zone Variable Air Volume,"Low Gas Heat, 1 Stage",208 VAC - 230 VAC,240,169000,135000,169000,135000,90,72,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5ML1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Low_Heat_230V,148000,13,Variable Air Volume,"Low Gas Heat, 1 Stage",208 VAC - 230 VAC,240,169000,135000,169000,135000,90,72,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VL1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Standard_Heat_230V,148000,13,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage",208 VAC - 230 VAC,240,260000,211000,85000,211000,90,72,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MS1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Standard_Heat_230V,148000,13,Variable Air Volume,"Standard Gas Heat, 2 Stage",208 VAC - 230 VAC,240,260000,211000,85000,211000,90,72,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VS1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Medium_Heat_230V,148000,13,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage",208 VAC - 230 VAC,240,360000,292000,117000,292000,90,72,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MM1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Medium_Heat_230V,148000,13,Variable Air Volume,"Medium Gas Heat, 2 Stage",208 VAC - 230 VAC,240,360000,292000,117000,292000,90,72,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VM1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_High_Heat_230V,148000,13,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage",208 VAC - 230 VAC,240,480000,389000,156000,389000,90,72,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MH1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_High_Heat_230V,148000,13,Variable Air Volume,"High Gas Heat, 2 Stage",208 VAC - 230 VAC,240,480000,389000,156000,389000,90,72,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VH1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Low_Heat_460V,148000,13,Single-Zone Variable Air Volume,"Low Gas Heat, 1 Stage",460 VAC,480,169000,135000,169000,135000,40,33,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5ML1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Low_Heat_460V,148000,13,Variable Air Volume,"Low Gas Heat, 1 Stage",460 VAC,480,169000,135000,169000,135000,40,33,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VL1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Standard_Heat_460V,148000,13,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage",460 VAC,480,260000,211000,85000,211000,40,33,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MS1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Standard_Heat_460V,148000,13,Variable Air Volume,"Standard Gas Heat, 2 Stage",460 VAC,480,260000,211000,85000,211000,40,33,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VS1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Medium_Heat_460V,148000,13,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage",460 VAC,480,360000,292000,117000,292000,40,33,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MM1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Medium_Heat_460V,148000,13,Variable Air Volume,"Medium Gas Heat, 2 Stage",460 VAC,480,360000,292000,117000,292000,40,33,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VM1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_High_Heat_460V,148000,13,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage",460 VAC,480,480000,389000,156000,389000,40,33,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MH1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_High_Heat_460V,148000,13,Variable Air Volume,"High Gas Heat, 2 Stage",460 VAC,480,480000,389000,156000,389000,40,33,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VH1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Low_Heat_575V,148000,13,Single-Zone Variable Air Volume,"Low Gas Heat, 1 Stage",575 VAC,600,169000,135000,169000,135000,30,25,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5ML1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Low_Heat_575V,148000,13,Variable Air Volume,"Low Gas Heat, 1 Stage",575 VAC,600,169000,135000,169000,135000,30,25,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VL1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Standard_Heat_575V,148000,13,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage",575 VAC,600,260000,211000,85000,211000,30,25,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MS1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Standard_Heat_575V,148000,13,Variable Air Volume,"Standard Gas Heat, 2 Stage",575 VAC,600,260000,211000,85000,211000,30,25,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VS1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Medium_Heat_575V,148000,13,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage",575 VAC,600,360000,292000,117000,292000,30,25,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MM1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Medium_Heat_575V,148000,13,Variable Air Volume,"Medium Gas Heat, 2 Stage",575 VAC,600,360000,292000,117000,292000,30,25,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VM1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_High_Heat_575V,148000,13,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage",575 VAC,600,480000,389000,156000,389000,30,25,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MH1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_High_Heat_575V,148000,13,Variable Air Volume,"High Gas Heat, 2 Stage",575 VAC,600,480000,389000,156000,389000,30,25,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VH1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Low_Heat_230V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"Low Gas Heat, 1 Stage",208 VAC - 230 VAC,240,169000,135000,169000,135000,90,72,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5ML1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Low_Heat_230V_w/Power_Exhaust,148000,13,Variable Air Volume,"Low Gas Heat, 1 Stage",208 VAC - 230 VAC,240,169000,135000,169000,135000,90,72,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VL1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Standard_Heat_230V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage",208 VAC - 230 VAC,240,260000,211000,85000,211000,90,72,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MS1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Standard_Heat_230V_w/Power_Exhaust,148000,13,Variable Air Volume,"Standard Gas Heat, 2 Stage",208 VAC - 230 VAC,240,260000,211000,85000,211000,90,72,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VS1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Medium_Heat_230V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage",208 VAC - 230 VAC,240,360000,292000,117000,292000,90,72,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MM1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Medium_Heat_230V_w/Power_Exhaust,148000,13,Variable Air Volume,"Medium Gas Heat, 2 Stage",208 VAC - 230 VAC,240,360000,292000,117000,292000,90,72,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VM1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_High_Heat_230V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage",208 VAC - 230 VAC,240,480000,389000,156000,389000,90,72,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MH1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_High_Heat_230V_w/Power_Exhaust,148000,13,Variable Air Volume,"High Gas Heat, 2 Stage",208 VAC - 230 VAC,240,480000,389000,156000,389000,90,72,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VH1Y,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Low_Heat_460V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"Low Gas Heat, 1 Stage",460 VAC,480,169000,135000,169000,135000,40,33,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5ML1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Low_Heat_460V_w/Power_Exhaust,148000,13,Variable Air Volume,"Low Gas Heat, 1 Stage",460 VAC,480,169000,135000,169000,135000,40,33,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VL1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Standard_Heat_460V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage",460 VAC,480,260000,211000,85000,211000,40,33,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MS1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Standard_Heat_460V_w/Power_Exhaust,148000,13,Variable Air Volume,"Standard Gas Heat, 2 Stage",460 VAC,480,260000,211000,85000,211000,40,33,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VS1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Medium_Heat_460V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage",460 VAC,480,360000,292000,117000,292000,40,33,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MM1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Medium_Heat_460V_w/Power_Exhaust,148000,13,Variable Air Volume,"Medium Gas Heat, 2 Stage",460 VAC,480,360000,292000,117000,292000,40,33,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VM1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_High_Heat_460V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage",460 VAC,480,480000,389000,156000,389000,40,33,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MH1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_High_Heat_460V_w/Power_Exhaust,148000,13,Variable Air Volume,"High Gas Heat, 2 Stage",460 VAC,480,480000,389000,156000,389000,40,33,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VH1G,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Low_Heat_575V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"Low Gas Heat, 1 Stage",575 VAC,600,169000,135000,169000,135000,30,25,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5ML1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Low_Heat_575V_w/Power_Exhaust,148000,13,Variable Air Volume,"Low Gas Heat, 1 Stage",575 VAC,600,169000,135000,169000,135000,30,25,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VL1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Standard_Heat_575V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage",575 VAC,600,260000,211000,85000,211000,30,25,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MS1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Standard_Heat_575V_w/Power_Exhaust,148000,13,Variable Air Volume,"Standard Gas Heat, 2 Stage",575 VAC,600,260000,211000,85000,211000,30,25,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VS1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_Medium_Heat_575V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage",575 VAC,600,360000,292000,117000,292000,30,25,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MM1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_Medium_Heat_575V_w/Power_Exhaust,148000,13,Variable Air Volume,"Medium Gas Heat, 2 Stage",575 VAC,600,360000,292000,117000,292000,30,25,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VM1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_Single-Zone_VAV_Blower_High_Heat_575V_w/Power_Exhaust,148000,13,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage",575 VAC,600,480000,389000,156000,389000,30,25,12,15.4,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5MH1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
13Ton_High_Efficiency_VAV_Blower_High_Heat_575V_w/Power_Exhaust,148000,13,Variable Air Volume,"High Gas Heat, 2 Stage",575 VAC,600,480000,389000,156000,389000,30,25,12,15,1044,60,3,1,1,90.125,54.25,106.5,Belt Drive,Single-Scroll & Two-Stage Scroll,Packaged Gas / Electric Rooftop Units - High Efficiency,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT156H5VH1J,R-454B,ASHRAE 90.1 Compliant,36,1,36,60,36,45,66,41,3.25,5.625,28.375,8.25,15,60.5,12.375,4.25,20,28,4.5,12.375,18,4,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,10.25
