,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Fan Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,System Performance EER##other##,System Performance IEER##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Model Number##other##,Refrigerant Used##other##,Standards##other##,Base Rail Height##length##inches,Bottom Drain Connection Vertical Offset##length##inches,Evaporator Side Service Clearance##length##inches,Front Side Service Clearance##length##inches,Minimum Operation Clearance##length##inches,Service Clearance##length##inches,Downflow Return Duct Vertical Offset##length##inches,Downflow Supply Duct Vertical Offset##length##inches,Downflow Return Air Connection Height##hvac_duct_size##inches,Downflow Return Air Connection Width##hvac_duct_size##inches,Downflow Return Duct Horizontal Offset##length##inches,Downflow Supply Air Connection Height##hvac_duct_size##inches,Downflow Supply Air Connection Width##hvac_duct_size##inches,Downflow Supply Duct Horizontal Offset##length##inches,Drain Connection Horizontal Offset##length##inches,Drain Connection Vertical Offset##length##inches,Enclosure Depth##length##inches,Enclosure Width##length##inches,Horizontal Return Air Connection Height##hvac_duct_size##inches,Horizontal Return Air Connection Width##hvac_duct_size##inches,Horizontal Return Duct Horizontal Offset##length##inches,Horizontal Return Duct Vertical Offset##length##inches,Horizontal Supply Air Connection Height##hvac_duct_size##inches,Horizontal Supply Air Connection Width##hvac_duct_size##inches,Horizontal Supply Duct Horizontal Offset##length##inches,Horizontal Supply Duct Vertical Offset##length##inches,Outdoor Fan Diameter##length##inches
7.5Ton_Standard_Efficiency_230V,89000,7.5,MSAV Multi-Stage Air Volume,208 VAC - 230 VAC,240,11,15,3750,1750,1209,60,3,1,60.125,46.875,101.25,Belt Drive,Singe-Stage & Two-Stage Scroll Compressor,Standard Efficiency Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,LHX092S5MN1Y,R-454B,ASHRAE 90.1 Compliant,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
7.5Ton_Standard_Efficiency_460V,89000,7.5,MSAV Multi-Stage Air Volume,460 VAC,480,11,15,3750,1750,1209,60,3,1,60.125,46.875,101.25,Belt Drive,Singe-Stage & Two-Stage Scroll Compressor,Standard Efficiency Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,LHX092S5MN1G,R-454B,ASHRAE 90.1 Compliant,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
7.5Ton_Standard_Efficiency_575V,89000,7.5,MSAV Multi-Stage Air Volume,575 VAC,600,11,15,3750,1750,1209,60,3,1,60.125,46.875,101.25,Belt Drive,Singe-Stage & Two-Stage Scroll Compressor,Standard Efficiency Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,LHX092S5MN1J,R-454B,ASHRAE 90.1 Compliant,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
8.5Ton_Standard_Efficiency_230V,100000,8.5,MSAV Multi-Stage Air Volume,208 VAC - 230 VAC,240,11,15,5000,1750,1241,60,3,1,60.125,46.875,101.25,Belt Drive,Singe-Stage & Two-Stage Scroll Compressor,Standard Efficiency Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,LHX102S5MN1Y,R-454B,ASHRAE 90.1 Compliant,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
8.5Ton_Standard_Efficiency_460V,100000,8.5,MSAV Multi-Stage Air Volume,460 VAC,480,11,15,5000,1750,1241,60,3,1,60.125,46.875,101.25,Belt Drive,Singe-Stage & Two-Stage Scroll Compressor,Standard Efficiency Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,LHX102S5MN1G,R-454B,ASHRAE 90.1 Compliant,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
8.5Ton_Standard_Efficiency_575V,100000,8.5,MSAV Multi-Stage Air Volume,575 VAC,600,11,15,5000,1750,1241,60,3,1,60.125,46.875,101.25,Belt Drive,Singe-Stage & Two-Stage Scroll Compressor,Standard Efficiency Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,LHX102S5MN1J,R-454B,ASHRAE 90.1 Compliant,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
10Ton_Standard_Efficiency_230V,116000,10,MSAV Multi-Stage Air Volume,208 VAC - 230 VAC,240,11,15,5000,1750,1314,60,3,1,60.125,46.875,101.25,Belt Drive,Singe-Stage & Two-Stage Scroll Compressor,Standard Efficiency Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,LHX120S5MN1Y,R-454B,ASHRAE 90.1 Compliant,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
10Ton_Standard_Efficiency_460V,116000,10,MSAV Multi-Stage Air Volume,460 VAC,480,11,15,5000,1750,1314,60,3,1,60.125,46.875,101.25,Belt Drive,Singe-Stage & Two-Stage Scroll Compressor,Standard Efficiency Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,LHX120S5MN1G,R-454B,ASHRAE 90.1 Compliant,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
10Ton_Standard_Efficiency_575V,116000,10,MSAV Multi-Stage Air Volume,575 VAC,600,11,15,5000,1750,1314,60,3,1,60.125,46.875,101.25,Belt Drive,Singe-Stage & Two-Stage Scroll Compressor,Standard Efficiency Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/k-series,K-Series,LHX,LHX120S5MN1J,R-454B,ASHRAE 90.1 Compliant,3.5,7,60,60,36,36,6.125,5.625,27,24,6.125,20,28,10.75,34.875,5.375,58.125,99.25,30,15.5,1.625,12.125,15.5,30,31.5,6.125,24
