,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Fan Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,System Performance EER##other##,System Performance IEER##other##,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Refrigerant Used##other##,Standards##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Service Clearance##length##inches,Minimum Operation Clearance##length##inches,Front Side Service Clearance##length##inches,Front Side Minimum Operation Clearance##length##inches,Evaporator Side Service Clearance##length##inches,Evaporator Side Minimum Operation Clearance##length##inches,Base Rail Height##length##inches,Bottom Drain Connection Horizontal Offset##length##inches,Bottom Drain Connection Vertical Offset##length##inches,Downflow Return Air Connection Height##hvac_duct_size##inches,Downflow Return Air Connection Width##hvac_duct_size##inches,Downflow Return Duct Horizontal Offset##length##inches,Downflow Return Duct Vertical Offset##length##inches,Downflow Supply Air Connection Height##hvac_duct_size##inches,Downflow Supply Air Connection Width##hvac_duct_size##inches,Downflow Supply Duct Horizontal Center Offset##length##inches,Downflow Supply Duct Horizontal Offset##length##inches,Downflow Supply Duct Vertical Offset##length##inches,Horizontal Return Air Connection Height##hvac_duct_size##inches,Horizontal Return Air Connection Width##hvac_duct_size##inches,Horizontal Return Duct Horizontal Offset##length##inches,Horizontal Return Duct Vertical Offset##length##inches,Horizontal Roof Curb Depth##length##inches,Horizontal Roof Curb Width##length##inches,Horizontal Supply Air Connection Width##hvac_duct_size##inches,Outdoor Fan Diameter##length##inches,Side Drain Connection Horizontal Offset##length##inches,Side Drain Connection Vertical Offset##length##inches,Unit Base Width##length##inches,TonV##other##
15Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_230V,172000,15,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,12.2,15.6,1026,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
17.5Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_230V,200000,17.5,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,12.2,16.2,1229,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
20Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_230V,228000,20,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,12.2,15.6,1243,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
25Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_230V,270000,25,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,10.8,14.5,1266,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
15Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_460V,172000,15,Single-Zone Variable Air Volume,460 VAC,480,12.2,15.6,1026,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
17.5Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_460V,200000,17.5,Single-Zone Variable Air Volume,460 VAC,480,12.2,16.2,1229,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
20Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_460V,228000,20,Single-Zone Variable Air Volume,460 VAC,480,12.2,15.6,1243,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
25Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_460V,270000,25,Single-Zone Variable Air Volume,460 VAC,480,10.8,14.5,1266,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
15Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_575V,172000,15,Single-Zone Variable Air Volume,575 VAC,600,12.2,15.6,1026,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
17.5Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_575V,200000,17.5,Single-Zone Variable Air Volume,575 VAC,600,12.2,16.2,1229,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
20Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_575V,228000,20,Single-Zone Variable Air Volume,575 VAC,600,12.2,15.6,1243,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
25Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_575V,270000,25,Single-Zone Variable Air Volume,575 VAC,600,10.8,14.5,1266,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
15Ton_VAV_Blower_High_Cooling_Efficiency_230V,172000,15,Variable Air Volume,208 VAC - 230 VAC,240,12.2,15.2,1026,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
17.5Ton_VAV_Blower_High_Cooling_Efficiency_230V,200000,17.5,Variable Air Volume,208 VAC - 230 VAC,240,12.2,15.7,1229,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
20Ton_VAV_Blower_High_Cooling_Efficiency_230V,228000,20,Variable Air Volume,208 VAC - 230 VAC,240,12.2,15.4,1243,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
25Ton_VAV_Blower_High_Cooling_Efficiency_230V,270000,25,Variable Air Volume,208 VAC - 230 VAC,240,10.8,14.5,1266,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
15Ton_VAV_Blower_High_Cooling_Efficiency_460V,172000,15,Variable Air Volume,460 VAC,480,12.2,15.2,1026,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
17.5Ton_VAV_Blower_High_Cooling_Efficiency_460V,200000,17.5,Variable Air Volume,460 VAC,480,12.2,15.7,1229,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
20Ton_VAV_Blower_High_Cooling_Efficiency_460V,228000,20,Variable Air Volume,460 VAC,480,12.2,15.4,1243,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
25Ton_VAV_Blower_High_Cooling_Efficiency_460V,270000,25,Variable Air Volume,460 VAC,480,10.8,14.5,1266,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
15Ton_VAV_Blower_High_Cooling_Efficiency_600V,172000,15,Variable Air Volume,575 VAC,600,12.2,15.2,1026,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
17.5Ton_VAV_Blower_High_Cooling_Efficiency_600V,200000,17.5,Variable Air Volume,575 VAC,600,12.2,15.7,1229,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
20Ton_VAV_Blower_High_Cooling_Efficiency_600V,228000,20,Variable Air Volume,575 VAC,600,12.2,15.4,1243,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
25Ton_VAV_Blower_High_Cooling_Efficiency_600V,270000,25,Variable Air Volume,575 VAC,600,10.8,14.5,1266,60,3,1,90.125,54.25,132 5/8,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,11000,2750,36,36,60,45,66,41,3.25,5.625,28.375,15,60.5,12.375,4.25,20,28,4.5,12.375,18,15,60.5,12.375,2,82.625,98.5,75,24,28.75,5.375,107.75,A
25Ton(302)_Single-Zone_VAV_Blower_High_Cooling_Efficiency_230V,300000,25,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,11.4,14.3,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
30Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_230V,350000,30,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,10.8,13.5,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
25Ton(302)_Single-Zone_VAV_Blower_High_Cooling_Efficiency_460V,300000,25,Single-Zone Variable Air Volume,460 VAC,480,11.4,14.3,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
30Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_460V,350000,30,Single-Zone Variable Air Volume,460 VAC,480,10.8,13.5,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
25Ton(302)_Single-Zone_VAV_Blower_High_Cooling_Efficiency_575V,300000,25,Single-Zone Variable Air Volume,575 VAC,600,11.4,14.3,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
30Ton_Single-Zone_VAV_Blower_High_Cooling_Efficiency_575V,350000,30,Single-Zone Variable Air Volume,575 VAC,600,10.8,13.5,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
25Ton(302)__VAV_Blower_High_Cooling_Efficiency_230V,300000,25,Variable Air Volume,208 VAC - 230 VAC,240,11.4,15.8,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
30Ton_Single-Zone_VAV_VAV_Blower_High_Cooling_Efficiency_230V,350000,30,Variable Air Volume,208 VAC - 230 VAC,240,10.8,14.2,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
25Ton(302)_VAV_Blower_High_Cooling_Efficiency_460V,300000,25,Variable Air Volume,460 VAC,480,11.4,15.8,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
30Ton_Single-Zone_VAV_VAV_Blower_High_Cooling_Efficiency_460V,350000,30,Variable Air Volume,460 VAC,480,10.8,14.2,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
25Ton(302)_VAV_Blower_High_Cooling_Efficiency_575V,300000,25,Variable Air Volume,575 VAC,600,11.4,15.8,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
30Ton_VAV_Blower_High_Cooling_Efficiency_575V,350000,30,Variable Air Volume,575 VAC,600,10.8,14.2,1592,60,3,1,90.125,65,145,Belt Drive,Scroll,Packaged Electric High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,15000,4000,36,36,60,45,66,41,3.25,5.625,28.375,15,78.5,17.5,4.25,20,28,4.5,17.5,18,15,78.5,12.375,2,82.625,98.5,75,24,31.5,5.375,119.75,B
