,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Fan Type##other##,Heating Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,Maximum Heating Input (MBH)##number##general,Maximum Heating Output (MBH)##number##general,Minimum Heating Input (MBH)##number##general,Minimum Heating Output (MBH)##number##general,System Performance EER##other##,System Performance EER2##other##,System Performance IEER##other##,System Performance SEER##other##,System Performance SEER2##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Gas Connection Size##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Model Number##other##,Refrigerant Used##other##,Standards##other##,Base Rail Height##length##inches,Bottom Drain Connection Vertical Offset##length##inches,Minimum Operation Clearance##length##inches,Service Clearance##length##inches,Clearance to Combustibles##length##inches,Front Side Service Clearance##length##inches,Front Side Clearance to Combustibles##length##inches,Downflow Duct Vertical Offset##length##inches,Downflow Return Air Connection Height##hvac_duct_size##inches,Downflow Return Air Connection Width##hvac_duct_size##inches,Downflow Return Duct Horizontal Offset##length##inches,Downflow Supply Air Connection Height##hvac_duct_size##inches,Downflow Supply Air Connection Width##hvac_duct_size##inches,Downflow Supply Duct Horizontal Offset##length##inches,Drain Connection Horizontal Offset##length##inches,Drain Connection Vertical Offset##length##inches,Enclosure Depth##length##inches,Enclosure Width##length##inches,Horizontal Return Air Connection Height##hvac_duct_size##inches,Horizontal Return Air Connection Width##hvac_duct_size##inches,Horizontal Return Duct Horizontal Offset##length##inches,Horizontal Return Duct Vertical Offset##length##inches,Horizontal Supply Air Connection Height##hvac_duct_size##inches,Horizontal Supply Air Connection Width##hvac_duct_size##inches,Horizontal Supply Duct Horizontal Offset##length##inches,Horizontal Supply Duct Vertical Offset##length##inches,Outdoor Fan Diameter##length##inches,Gas Connection Horizontal Offset##length##inches,Gas Connection Vertical Offset##length##inches
3Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,36000,3,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,13.5,N/A,N/A,17.5,1200,800,375,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT036H5EB1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,49000,4,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EB1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,60000,5,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EB1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,36000,3,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,13.5,N/A,N/A,17.5,1200,800,375,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT036H5EQ1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,49000,4,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EQ1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,60000,5,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EQ1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,49000,4,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EX1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,60000,5,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EX1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,36000,3,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,13.5,N/A,N/A,17.5,1200,800,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT036H5EB1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,49000,4,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EB1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,60000,5,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EB1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,69000,6,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,12.2,N/A,17.3,N/A,N/A,2000,1500,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT072H5EB1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,36000,3,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,13.5,N/A,N/A,17.5,1200,800,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT036H5EQ1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,49000,4,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EQ1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,60000,5,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EQ1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,69000,6,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,12.2,N/A,17.3,N/A,N/A,2000,1500,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT072H5EQ1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,49000,4,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EX1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,60000,5,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EX1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,69000,6,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,12.2,N/A,17.3,N/A,N/A,2000,1500,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT072H5EX1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Standard_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,36000,3,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",460 VAC,480,65000,52000,53000,43000,N/A,13.5,N/A,N/A,17.5,1200,800,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT036H5EB1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Standard_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,49000,4,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",460 VAC,480,65000,52000,53000,43000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EB1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Standard_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,60000,5,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",460 VAC,480,65000,52000,53000,43000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EB1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Standard_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,69000,6,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",460 VAC,480,65000,52000,53000,43000,12.2,N/A,17.3,N/A,N/A,2000,1500,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT072H5EB1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Medium_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,36000,3,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",460 VAC,480,108000,87000,81000,66000,N/A,13.5,N/A,N/A,17.5,1200,800,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT036H5EQ1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Medium_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,49000,4,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",460 VAC,480,108000,87000,81000,66000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EQ1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Medium_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,60000,5,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",460 VAC,480,108000,87000,81000,66000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EQ1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Medium_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,69000,6,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",460 VAC,480,108000,87000,81000,66000,12.2,N/A,17.3,N/A,N/A,2000,1500,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT072H5EQ1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_High_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,49000,4,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",460 VAC,480,150000,121000,113000,92000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EX1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_High_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,60000,5,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",460 VAC,480,150000,121000,113000,92000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EX1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_High_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,69000,6,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",460 VAC,480,150000,121000,113000,92000,12.2,N/A,17.3,N/A,N/A,2000,1500,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT072H5EX1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Standard_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,36000,3,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",575 VAC,600,65000,52000,53000,43000,N/A,13.5,N/A,N/A,17.5,1200,800,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT036H5EB1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Standard_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,49000,4,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",575 VAC,600,65000,52000,53000,43000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EB1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Standard_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,60000,5,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",575 VAC,600,65000,52000,53000,43000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EB1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Standard_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,69000,6,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",575 VAC,600,65000,52000,53000,43000,12.2,N/A,17.3,N/A,N/A,2000,1500,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT072H5EB1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Medium_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,36000,3,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",575 VAC,600,108000,87000,81000,66000,N/A,13.5,N/A,N/A,17.5,1200,800,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT036H5EQ1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Medium_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,49000,4,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",575 VAC,600,108000,87000,81000,66000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EQ1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Medium_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,60000,5,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",575 VAC,600,108000,87000,81000,66000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EQ1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Medium_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,69000,6,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",575 VAC,600,108000,87000,81000,66000,12.2,N/A,17.3,N/A,N/A,2000,1500,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT072H5EQ1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_High_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,49000,4,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",575 VAC,600,150000,121000,113000,92000,N/A,13,N/A,N/A,17.3,1600,1200,375,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT048H5EX1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_High_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,60000,5,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",575 VAC,600,150000,121000,113000,92000,N/A,12.5,N/A,N/A,16.4,1800,1350,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT060H5EX1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_High_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,69000,6,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",575 VAC,600,150000,121000,113000,92000,12.2,N/A,17.3,N/A,N/A,2000,1500,376,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Gas Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LGT,LGT072H5EX1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
