,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Nominal Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,High Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,Fan Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,System Performance EER##other##,System Performance IEER##other##,COP At 17F##other##,COP At 47F##other##,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Refrigerant Used##other##,Standards##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_230V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,11.1,15.2,2.1,3.4,619,60,3,1,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5520,2400
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_460V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,460 VAC,480,11.1,15.2,2.1,3.4,619,60,3,1,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5520,2400
12.5Ton_High_Efficiency_Single-Zone_VAV_Blower_575V,140000,12.5,73000,128000,Single-Zone Variable Air Volume,575 VAC,600,11.1,15.2,2.1,3.4,619,60,3,1,60.25,46.875,130,Direct Drive,Single-Stage & Two-Stage Scroll,Packaged Heat Pump Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LHT,R-454B,ASHRAE 90.1 Compliant,5520,2400
