  ,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Nominal Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,Total Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,Fan Type##other##,Heating Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,Maximum Heating Input (MBH)##number##general,Maximum Heating Output (MBH)##number##general,Minimum Heating Input (MBH)##number##general,Minimum Heating Output (MBH)##number##general,System Performance EER##other##,System Performance EER2##other##,System Performance IEER##other##,System Performance SEER2##other##,System Performance HSPF2##other##,COP At 17F##other##,COP At 47F##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Gas Connection Size##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Model Number##other##,Refrigerant Used##other##,Standards##other##,Base Rail Height##length##inches,Bottom Drain Connection Vertical Offset##length##inches,Minimum Operation Clearance##length##inches,Service Clearance##length##inches,Clearance to Combustibles##length##inches,Front Side Service Clearance##length##inches,Front Side Clearance to Combustibles##length##inches,Downflow Duct Vertical Offset##length##inches,Downflow Return Air Connection Height##hvac_duct_size##inches,Downflow Return Air Connection Width##hvac_duct_size##inches,Downflow Return Duct Horizontal Offset##length##inches,Downflow Supply Air Connection Height##hvac_duct_size##inches,Downflow Supply Air Connection Width##hvac_duct_size##inches,Downflow Supply Duct Horizontal Offset##length##inches,Drain Connection Horizontal Offset##length##inches,Drain Connection Vertical Offset##length##inches,Enclosure Depth##length##inches,Enclosure Width##length##inches,Horizontal Return Air Connection Height##hvac_duct_size##inches,Horizontal Return Air Connection Width##hvac_duct_size##inches,Horizontal Return Duct Horizontal Offset##length##inches,Horizontal Return Duct Vertical Offset##length##inches,Horizontal Supply Air Connection Height##hvac_duct_size##inches,Horizontal Supply Air Connection Width##hvac_duct_size##inches,Horizontal Supply Duct Horizontal Offset##length##inches,Horizontal Supply Duct Vertical Offset##length##inches,Outdoor Fan Diameter##length##inches,Gas Connection Horizontal Offset##length##inches,Gas Connection Vertical Offset##length##inches
3Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,38000,3,19000,34000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,12.2,N/A,16,7.2,2.1,3.5,1400,935,368,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT036H5EB1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,46800,4,25000,44000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,367,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EB1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,60000,5,33000,57000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EB1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,38000,3,19000,34000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,12.2,N/A,16,7.2,2.1,3.5,1400,935,368,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT036H5EQ1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,46800,4,25000,44000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,367,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EQ1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,60000,5,33000,57000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EQ1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,38000,4,19000,34000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,367,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EX1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_1Ph,46800,5,25000,44000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,N/A,11.8,N/A,15.6,7.2,2.1,3.5,1800,1300,381,60,1,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EX1P,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,38000,3,19000,34000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,12.2,N/A,16,7.2,2.1,3.5,1400,935,369,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT036H5EB1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,46800,4,25000,44000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,368,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EB1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,60000,5,33000,57000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EB1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Standard_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,70000,6,35500,66000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,65000,52000,53000,43000,11,N/A,15.5,N/A,N/A,2.25,3.5,2100,1500,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT72H5EB1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,38000,3,19000,34000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,12.2,N/A,16,7.2,2.1,3.5,1400,935,369,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT036H5EQ1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,46800,4,25000,44000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,368,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EQ1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,60000,5,33000,57000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EQ1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Medium_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,70000,6,35500,66000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,108000,87000,81000,66000,11,N/A,15.5,N/A,N/A,2.25,3.5,2100,1500,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT72H5EQ1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,46800,4,19000,34000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,368,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EX1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,60000,5,25000,44000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EX1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_High_Gas_Heat_2_Stage_Low_Nox_230V_3Ph,70000,6,33000,57000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",208 VAC - 230 VAC,240,150000,121000,113000,92000,11,N/A,15.5,N/A,N/A,2.25,3.5,2100,1500,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT72H5EX1Y,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Standard_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,38000,3,19000,34000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",460 VAC,480,65000,52000,53000,43000,N/A,12.2,N/A,16,7.2,2.1,3.5,1400,935,369,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT036H5EB1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Standard_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,46800,4,25000,44000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",460 VAC,480,65000,52000,53000,43000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,368,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EB1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Standard_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,60000,5,33000,57000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",460 VAC,480,65000,52000,53000,43000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EB1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Standard_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,70000,6,35500,66000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",460 VAC,480,65000,52000,53000,43000,11,N/A,15.5,N/A,N/A,2.25,3.5,2100,1500,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT72H5EB1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Medium_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,38000,3,19000,34000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",460 VAC,480,108000,87000,81000,66000,N/A,12.2,N/A,16,7.2,2.1,3.5,1400,935,369,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT036H5EQ1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Medium_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,46800,4,25000,44000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",460 VAC,480,108000,87000,81000,66000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,368,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EQ1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Medium_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,60000,5,33000,57000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",460 VAC,480,108000,87000,81000,66000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EQ1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Medium_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,70000,6,35500,66000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",460 VAC,480,108000,87000,81000,66000,11,N/A,15.5,N/A,N/A,2.25,3.5,2100,1500,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT72H5EQ1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_High_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,46800,4,19000,34000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",460 VAC,480,150000,121000,113000,92000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,368,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EX1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_High_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,60000,5,25000,44000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",460 VAC,480,150000,121000,113000,92000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EX1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_High_Gas_Heat_2_Stage_Low_Nox_460V_3Ph,70000,6,33000,57000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",460 VAC,480,150000,121000,113000,92000,11,N/A,15.5,N/A,N/A,2.25,3.5,2100,1500,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT72H5EX1G,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Standard_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,38000,3,19000,34000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",575 VAC,600,65000,52000,53000,43000,N/A,12.2,N/A,16,7.2,2.1,3.5,1400,935,369,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT036H5EB1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Standard_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,46800,4,25000,44000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",575 VAC,600,65000,52000,53000,43000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,368,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EB1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Standard_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,60000,5,33000,57000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",575 VAC,600,65000,52000,53000,43000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EB1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Standard_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,70000,6,35500,66000,Single-Zone Variable Air Volume,"Standard Gas Heat, 2 Stage, Low Nox",575 VAC,600,65000,52000,53000,43000,11,N/A,15.5,N/A,N/A,2.25,3.5,2100,1500,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT72H5EB1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
3Ton_Medium_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,38000,3,19000,34000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",575 VAC,600,108000,87000,81000,66000,N/A,12.2,N/A,16,7.2,2.1,3.5,1400,935,369,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT036H5EQ1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_Medium_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,46800,4,25000,44000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",575 VAC,600,108000,87000,81000,66000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,368,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EQ1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_Medium_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,60000,5,33000,57000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",575 VAC,600,108000,87000,81000,66000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EQ1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_Medium_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,70000,6,35500,66000,Single-Zone Variable Air Volume,"Medium Gas Heat, 2 Stage, Low Nox",575 VAC,600,108000,87000,81000,66000,11,N/A,15.5,N/A,N/A,2.25,3.5,2100,1500,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT72H5EQ1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
4Ton_High_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,46800,4,19000,34000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",575 VAC,600,150000,121000,113000,92000,N/A,12,N/A,15.6,7.2,2.1,3.5,1400,1100,368,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT048H5EX1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
5Ton_High_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,60000,5,25000,44000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",575 VAC,600,150000,121000,113000,92000,N/A,11.8,N/A,15.2,7.2,2.2,3.5,1800,1300,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT060H5EX1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
6Ton_High_Gas_Heat_2_Stage_Low_Nox_575V_3Ph,70000,6,33000,57000,Single-Zone Variable Air Volume,"High Gas Heat, 2 Stage, Low Nox",575 VAC,600,150000,121000,113000,92000,11,N/A,15.5,N/A,N/A,2.25,3.5,2100,1500,381,60,3,1,0.5,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Dual Fuel High Efficiency Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LDT,LDT72H5EX1J,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,1,48,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24,27,15
