,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Enclosure Height##length##inches,Overall Width##length##inches,Overall Depth##length##inches,Model##other##,Model Number##other##,Minimum Circuit Amps##electrical_current##amperes,Nominal Cooling Capacity (Tons)##other##,Unit Weight##force##pounds_force,Description##other##,Sound Pressure Level_dBA##other##,Phase##other##,Frequency##electrical_frequency##hertz,Voltage Comments##other##,Voltage##electrical_potential##volts,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Refrigerant Charge##force##pounds_force,Maximum Overcurrent Protection##electrical_current##amperes,Compressor Rated Load Amps##electrical_current##amperes,Compressor Locked Rotor Amps##electrical_current##amperes,Refrigerant Used##other##,Lower Access Panel Depth##length##inches,Lower Access Panel Width##length##inches,Base Unit Height##length##inches,Standoff Height##length##inches,Standoff Offset A##length##inches,Standoff Offset B##length##inches,Suction Valve Height##length##inches,Clearance Length##length##inches,Enclosure Material##other##,URL##other##,Product Page URL##other##,Series##other##,Standards##other##
3Ton_ML14KP1-036-233A01 3 Phase,36000,32 1/2,32 1/4,32 1/4,ML14KP1,ML14KP1-036-233A01,15.4,3,220,Split System Heat Pump,75,3,60,208 VAC - 230 VAC,240, 3/8, 7/8,7.125,25,12.2,97.5,R-454B,4,7,33 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3.5Ton_ML14KP1-042-233A01 3 Phase,42000,36 1/2,32 1/4,32 1/4,ML14KP1,ML14KP1-042-233A01,12.3,3.5,250,Split System Heat Pump,78,3,60,208 VAC - 230 VAC,240, 3/8, 7/8,8.3125,20,9.6,90,R-454B,4,7,37 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_ML14KP1-048-233A01 3 Phase,48000,36 1/2,32 1/4,32 1/4,ML14KP1,ML14KP1-048-233A01,16.4,4,250,Split System Heat Pump,79,3,60,208 VAC - 230 VAC,240, 3/8, 7/8,8.375,25,12.8,120.4,R-454B,4,7,37 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_ML14KP1-060-233A01 3 Phase,60000,42 1/2,32 1/4,32 1/4,ML14KP1,ML14KP1-060-233A01,20.4,5,260,Split System Heat Pump,79,3,60,208 VAC - 230 VAC,240, 3/8,1 1/8,9.375,35,16,156.4,R-454B,4,7,43 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3Ton_ML14KP1-036-463A01 3 Phase,36000,32 1/2,32 1/4,32 1/4,ML14KP1,ML14KP1-036-463A01,7.4,3,220,Split System Heat Pump,75,3,60,460 VAC,480, 3/8, 7/8,7.125,10,5.8,44.3,R-454B,4,7,33 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3.5Ton_ML14KP1-042-463A01 3 Phase,42000,36 1/2,32 1/4,32 1/4,ML14KP1,ML14KP1-042-463A01,6.5,3.5,250,Split System Heat Pump,78,3,60,460 VAC,480, 3/8, 7/8,8.3125,10,4.9,36,R-454B,4,7,37 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_ML14KP1-048-463A01 3 Phase,48000,36 1/2,32 1/4,32 1/4,ML14KP1,ML14KP1-048-463A01,7.9,4,250,Split System Heat Pump,79,3,60,460 VAC,480, 3/8, 7/8,8.375,10,6,49.4,R-454B,4,7,37 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_ML14KP1-060-463A01 3 Phase,60000,42 1/2,32 1/4,32 1/4,ML14KP1,ML14KP1-060-463A01,9.1,5,260,Split System Heat Pump,79,3,60,460 VAC,480, 3/8,1 1/8,9.375,15,7.1,69,R-454B,4,7,43 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
