,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Enclosure Height##length##inches,Overall Width##length##inches,Overall Depth##length##inches,Model##other##,Model Number##other##,Minimum Circuit Amps##electrical_current##amperes,Nominal Cooling Capacity (Tons)##other##,Unit Weight##force##pounds_force,Description##other##,Sound Pressure Level_dBA##other##,Phase##other##,Frequency##electrical_frequency##hertz,Voltage Comments##other##,Voltage##electrical_potential##volts,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Refrigerant Charge##force##pounds_force,Maximum Overcurrent Protection##electrical_current##amperes,Compressor Rated Load Amps##electrical_current##amperes,Compressor Locked Rotor Amps##electrical_current##amperes,Refrigerant Used##other##,Lower Access Panel Depth##length##inches,Lower Access Panel Width##length##inches,Base Unit Height##length##inches,Standoff Height##length##inches,Standoff Offset A##length##inches,Standoff Offset B##length##inches,Suction Valve Height##length##inches,Clearance Length##length##inches,Enclosure Material##other##,URL##other##,Product Page URL##other##,Series##other##,Standards##other##
3Ton_ML13KC1-036-233A01 3 Phase,36000,32 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-036-233A01,17,3,161,Split System Air Conditioner,76,3,60,208 VAC - 230 VAC,240, 3/8, 7/8,5.625,25,12.8,97.5,R-454B,4,7,33 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3.5Ton_ML13KC1-042-233A01 3 Phase,42000,36 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-042-233A01,17.8,3.5,195,Split System Air Conditioner,76,3,60,208 VAC - 230 VAC,240, 3/8, 7/8,6.125,25,12.2,102.8,R-454B,4,7,37 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_ML13KC1-048-233A01 3 Phase,48000,28 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-048-233A01,16.9,4,215,Split System Air Conditioner,78,3,60,208 VAC - 230 VAC,240, 3/8, 7/8,7.625,25,12.2,120.4,R-454B,4,7,29 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_ML13KC1-060-233A01 3 Phase,60000,36 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-060-233A01,21.7,5,218,Split System Air Conditioner,80,3,60,208 VAC - 230 VAC,240, 3/8,1 1/8,6.5,35,16,156.4,R-454B,4,7,37 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3Ton_ML13KC1-036-463A01 3 Phase,36000,32 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-036-463A01,6.9,3,161,Split System Air Conditioner,76,3,60,460 VAC,480, 3/8, 7/8,5.625,10,5.1,44.3,R-454B,4,7,33 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3.5Ton_ML13KC1-042-463A01 3 Phase,42000,36 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-042-463A01,9.8,3.5,195,Split System Air Conditioner,76,3,60,460 VAC,480, 3/8, 7/8,6.125,15,5.8,50,R-454B,4,7,37 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_ML13KC1-048-463A01 3 Phase,48000,28 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-048-463A01,8.9,4,215,Split System Air Conditioner,78,3,60,460 VAC,480, 3/8, 7/8,7.625,15,6.4,50,R-454B,4,7,29 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_ML13KC1-060-463A01 3 Phase,60000,36 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-060-463A01,9.7,5,218,Split System Air Conditioner,80,3,60,460 VAC,480, 3/8,1 1/8,6.5,15,7,69,R-454B,4,7,37 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3Ton_ML13KC1-036-573A01 3 Phase,36000,32 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-036-573A01,6.1,3,161,Split System Air Conditioner,76,3,60,575 VAC,600, 3/8, 7/8,5.625,10,4.5,27.1,R-454B,4,7,33 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_ML13KC1-048-573A01 3 Phase,48000,28 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-048-573A01,7.1,4,215,Split System Air Conditioner,78,3,60,575 VAC,600, 3/8, 7/8,7.625,10,5.1,41,R-454B,4,7,29 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_ML13KC1-060-573A01 3 Phase,60000,36 1/2,28 1/4,28 1/4,ML13KC1,ML13KC1-060-573A01,8.7,5,218,Split System Air Conditioner,80,3,60,575 VAC,600, 3/8,1 1/8,6.5,15,6.4,47.8,R-454B,4,7,37 1/4,2,4 3/8,6 3/8,2,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
