,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Enclosure Height##length##inches,Overall Width##length##inches,Overall Depth##length##inches,Model##other##,Model Number##other##,Minimum Circuit Amps##electrical_current##amperes,Nominal Cooling Capacity (Tons)##other##,Unit Weight##force##pounds_force,Description##other##,Sound Pressure Level_dBA##other##,Phase##other##,Frequency##electrical_frequency##hertz,Voltage Comments##other##,Voltage##electrical_potential##volts,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Refrigerant Charge##force##pounds_force,Maximum Overcurrent Protection##electrical_current##amperes,Compressor Rated Load Amps##electrical_current##amperes,Compressor Locked Rotor Amps##electrical_current##amperes,Refrigerant Used##other##,Lower Access Panel Depth##length##inches,Lower Access Panel Width##length##inches,Base Unit Height##length##inches,Standoff Height##length##inches,Standoff Offset A##length##inches,Standoff Offset B##length##inches,Suction Valve Height##length##inches,Clearance Length##length##inches,Enclosure Material##other##,URL##other##,Product Page URL##other##,Series##other##,Standards##other##
3Ton_ML17KC2-036-233A01 3 Phase,36000,33,28 1/4,28.25,ML17KC2,ML17KC2-036-233A01,13.6,3,188,"Split Systems, Two-stage Compressor, 3 Phase",73,3,60,208 VAC - 230 VAC,240, 3/8, 7/8,6.5,20,9.9,82,R-454B,4,6,33 3/4,2,4 3/8,6 3/8,2 3/4,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/ ,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_ML17KC2-048-233A01 3 Phase,48000,33,32 1/4,32.25,ML17KC2,ML17KC2-048-233A01,17.6,4,206,"Split Systems, Two-stage Compressor, 3 Phase",74,3,60,208 VAC - 230 VAC,240, 3/8, 7/8,7.875,30,11.9,112,R-454B,4,6,33 3/4,2,4 3/8,6 3/8,2 3/4,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/ ,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_ML17KC2-060-233A01 3 Phase,60000,42 1/4,32 1/4,32.25,ML17KC2,ML17KC2-060-233A01,23.4,5,246,"Split Systems, Two-stage Compressor, 3 Phase",75,3,60,208 VAC - 230 VAC,240, 3/8,1 1/8,9.3125,40,13.8,150,R-454B,4,6,43 1/4,2,4 3/8,6 3/8,2 3/4,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/ ,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3Ton_ML17KC2-036-463A01 3 Phase,36000,33,28 1/4,28.25,ML17KC2,ML17KC2-036-463A01,6.5,3,188,"Split Systems, Two-stage Compressor, 3 Phase",73,3,60,460 VAC,480, 3/8, 7/8,6.5,15,4.8,44.3,R-454B,4,6,33 3/4,2,4 3/8,6 3/8,2 3/4,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/ ,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_ML17KC2-048-463A01 3 Phase,48000,33,32 1/4,32.25,ML17KC2,ML17KC2-048-463A01,9.9,4,206,"Split Systems, Two-stage Compressor, 3 Phase",74,3,60,460 VAC,480, 3/8, 7/8,7.875,15,6.8,61.8,R-454B,4,6,33 3/4,2,4 3/8,6 3/8,2 3/4,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/ ,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_ML17KC2-060-463A01 3 Phase,60000,42 1/4,32 1/4,32.25,ML17KC2,ML17KC2-060-463A01,11.5,5,246,"Split Systems, Two-stage Compressor, 3 Phase",75,3,60,460 VAC,480, 3/8,1 1/8,9.3125,15,6.9,58,R-454B,4,6,43 1/4,2,4 3/8,6 3/8,2 3/4,36,Metal - Allied - Steel - Warm Gray,https://www.allied-commercial.com/ ,https://www.allied-commercial.com/products/small-split-systems,MERIT®,AHRI Standard 210/240 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
