,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Voltage Comments##other##,Voltage##electrical_potential##volts,Unit Weight##force##pounds_force,Frequency##electrical_frequency##hertz,Condensate Drain Connection Diameter##pipe_size##inches,Overall Depth##length##inches,Enclosure Height##length##inches,Enclosure Width##length##inches,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Model Number##other##,Refrigerant Used##other##,Standards##other##,Supply Air Connection Width##hvac_duct_size##inches,Supply Air Connection Height##hvac_duct_size##inches,Return Air Connection Width##hvac_duct_size##inches,Return Air Connection Height##hvac_duct_size##inches,Coil Face Area##area##square_feet,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Fan Horsepower##electrical_power##horsepower,Fan Full Load Amps##electrical_current##amperes,Drain Upflow Vertical Offset##length##inches,Drain Downflow Vertical Offset##length##inches,Drain Horizontal Flow Vertical Offset##length##inches,Drain Vertical Flow Horizontal Offset 2##length##inches,Drain Horizontal Flow Horizontal Offset 2##length##inches,Drain Vertical Flow Horizontal Offset 1##length##inches,Drain Horizontal Flow Horizontal Offset 1##length##inches,Supply Air Outlet Vertical Offset##length##inches,Return Air Outlet Vertical Offset##length##inches,Refrigerant Suction Gas Connection Upflow Vertical Offset##length##inches,Refrigerant Suction Gas Connection Vertical Flow Horizontal Offset##length##inches,Refrigerant Suction Gas Connection Horizontal Flow Vertical Offset##length##inches,Refrigerant Suction Gas Connection Horizontal Flow Horizontal Offset##length##inches,Refrigerant Suction Gas Connection Downflow Vertical Offset##length##inches,Refrigerant Liquid Connection Upflow Vertical Offset##length##inches,Refrigerant Liquid Connection Downflow Vertical Offset##length##inches,Refrigerant Liquid Connection Horizontal Flow Vertical Offset##length##inches,Refrigerant Liquid Connection Vertical Flow Horizontal Offset##length##inches,Refrigerant Liquid Connection Horizontal Flow Horizontal Offset##length##inches
1.5Ton_7AH2AE18PX,18000,1.5,208 VAC - 230 VAC,240,137,60,0.75,20.625,49.25,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE18PX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,19,4.44,0.75,0.375,0.5,4.1,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
2Ton_7AH2AE24PX,24000,2,208 VAC - 230 VAC,240,137,60,0.75,20.625,49.25,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE24PX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,19,4.44,0.75,0.375,0.5,4.1,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
2.5Ton_7AH2AE30PX,30000,2.5,208 VAC - 230 VAC,240,150,60,0.75,22.625,51,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE30PX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,21,5,0.75,0.375,0.5,4.1,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
3Ton_7AH2AE36PX,36000,3,208 VAC - 230 VAC,240,150,60,0.75,22.625,51,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE36PX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,21,5,0.75,0.375,0.5,4.1,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
3Ton_7AH2AE36GX,36000,3,460 VAC,480,150,60,0.75,22.625,51,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE36GX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,21,5,0.75,0.375,0.5,4.1,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
3.5Ton_7AH2AE42PX,42000,3.5,208 VAC - 230 VAC,240,186,60,0.75,24.625,58.5,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE42PX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,23,7.22,0.75,0.375,1,7.6,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
4Ton_7AH2AE48PX,48000,4,208 VAC - 230 VAC,240,186,60,0.75,24.625,58.5,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE48PX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,23,7.22,0.75,0.375,1,7.6,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
4Ton_7AH2AE48GX,48000,4,460 VAC,480,186,60,0.75,24.625,58.5,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE48GX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,23,7.22,0.75,0.375,1,7.6,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
5Ton_7AH2AE60PX,60000,5,208 VAC - 230 VAC,240,199,60,0.75,24.625,62.5,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE60PX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,23,8.33,0.75,0.375,1,7.6,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
5Ton_7AH2AE60GX,60000,5,460 VAC,480,199,60,0.75,24.625,62.5,21.25,Air Handler - Upflow / Horizontal - High Efficiency Blower Motor,https://www.alliednow.com/products/air-handlers/7ah2ae,7AH2AE,7AH2AE,7AH2AE60GX-71,R-454B,AHRI 210/240; ISO 9001,19  3/4 ,11  1/16,20,23,8.33,0.75,0.375,1,7.6,2 3/4,1,1 1/2,5 1/4,7 1/2,3 1/2,5 3/4,0.75,0.63,7 5/8,5 1/2,5 1/2,7 3/8,5 5/8,5 5/8,3 5/8,4 3/8,4 3/8,5 3/8
