,Nominal Cooling Capacity (Tons)##other##,Unit Weight##force##pounds_force,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute
6Ton_EL072KASS,6,409,1200,3000
7.5Ton_EL090KASD,7.5,431,1600,3600
10Ton_EL120KASD,10,495,2000,4800
12.5Ton_EL150KASD,12.5,509,2600,6000
15Ton_EL180KASD,15,727,3200,7200
20Ton_EL240KASD,20,799,4200,8600
