,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Fan Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,System Performance EER##other##,System Performance EER2##other##,System Performance IEER##other##,System Performance SEER##other##,System Performance SEER2##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Refrigerant Used##other##,Standards##other##,Base Rail Height##length##inches,Bottom Drain Connection Vertical Offset##length##inches,Minimum Operation Clearance##length##inches,Service Clearance##length##inches,Downflow Duct Vertical Offset##length##inches,Downflow Return Air Connection Height##hvac_duct_size##inches,Downflow Return Air Connection Width##hvac_duct_size##inches,Downflow Return Duct Horizontal Offset##length##inches,Downflow Supply Air Connection Height##hvac_duct_size##inches,Downflow Supply Air Connection Width##hvac_duct_size##inches,Downflow Supply Duct Horizontal Offset##length##inches,Drain Connection Horizontal Offset##length##inches,Drain Connection Vertical Offset##length##inches,Enclosure Depth##length##inches,Enclosure Width##length##inches,Horizontal Return Air Connection Height##hvac_duct_size##inches,Horizontal Return Air Connection Width##hvac_duct_size##inches,Horizontal Return Duct Horizontal Offset##length##inches,Horizontal Return Duct Vertical Offset##length##inches,Horizontal Supply Air Connection Height##hvac_duct_size##inches,Horizontal Supply Air Connection Width##hvac_duct_size##inches,Horizontal Supply Duct Horizontal Offset##length##inches,Horizontal Supply Duct Vertical Offset##length##inches,Outdoor Fan Diameter##length##inches
3Ton_High_Efficiency_Single-Zone_VAV_230V_1Ph,36000,3,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,N/A,13.5,N/A,N/A,17.5,1200,800,366,60,1,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
4Ton_High_Efficiency_Single-Zone_VAV_230V_1Ph,49000,4,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,N/A,13,N/A,N/A,17.3,1600,1200,367,60,1,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
5Ton_High_Efficiency_Single-Zone_VAV_230V_1Ph,60000,5,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,N/A,12.5,N/A,N/A,16.4,1800,1350,367,60,1,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
3Ton_High_Efficiency_Single-Zone_VAV_230V_3Ph,36000,3,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,N/A,13.5,N/A,N/A,17.5,1200,800,366,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
4Ton_High_Efficiency_Single-Zone_VAV_230V_3Ph,49000,4,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,N/A,13,N/A,N/A,17.3,1600,1200,367,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
5Ton_High_Efficiency_Single-Zone_VAV_230V_3Ph,60000,5,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,N/A,12.5,N/A,N/A,16.4,1800,1350,367,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
6Ton_High_Efficiency_Single-Zone_VAV_230V_3Ph,69000,6,Single-Zone Variable Air Volume,208 VAC - 230 VAC,240,12.2,N/A,17.3,N/A,N/A,2000,1500,367,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
3Ton_High_Efficiency_Single-Zone_VAV_460V_3Ph,36000,3,Single-Zone Variable Air Volume,460 VAC,480,N/A,13.5,N/A,N/A,17.5,1200,800,366,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
4Ton_High_Efficiency_Single-Zone_VAV_460V_3Ph,49000,4,Single-Zone Variable Air Volume,460 VAC,480,N/A,13,N/A,N/A,17.3,1600,1200,367,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
5Ton_High_Efficiency_Single-Zone_VAV_460V_3Ph,60000,5,Single-Zone Variable Air Volume,460 VAC,480,N/A,12.5,N/A,N/A,16.4,1800,1350,367,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
6Ton_High_Efficiency_Single-Zone_VAV_460V_3Ph,69000,6,Single-Zone Variable Air Volume,460 VAC,480,12.2,N/A,17.3,N/A,N/A,2000,1500,367,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
3Ton_High_Efficiency_Single-Zone_VAV_575V_3Ph,36000,3,Single-Zone Variable Air Volume,575 VAC,600,N/A,13.5,N/A,N/A,17.5,1200,800,366,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
4Ton_High_Efficiency_Single-Zone_VAV_575V_3Ph,49000,4,Single-Zone Variable Air Volume,575 VAC,600,N/A,13,N/A,N/A,17.3,1600,1200,367,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
5Ton_High_Efficiency_Single-Zone_VAV_575V_3Ph,60000,5,Single-Zone Variable Air Volume,575 VAC,600,N/A,12.5,N/A,N/A,16.4,1800,1350,367,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
6Ton_High_Efficiency_Single-Zone_VAV_575V_3Ph,69000,6,Single-Zone Variable Air Volume,575 VAC,600,12.2,N/A,17.3,N/A,N/A,2000,1500,367,60,3,1,47,46.875,85.25,Direct Drive,Two-Stage Scroll Compressor,Packaged Electric Rooftop Units,https://www.allied-commercial.com/products/packaged-rooftop-units/e-series,E-Series,LCT,R-454B,ASHRAE 90.1 Compliant,3.5,6.625,36,36,7,29,11,5.625,20,18,16.25,26.5,5.5,45,83.25,29,11,2,5.5,20,19.5,18.375,5.5,24
