,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##number##general,Fan Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,System Performance EER##other##,System Performance IEER##other##,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Unit Weight##force##kilograms_force,Frequency##electrical_frequency##hertz,Phase##other##,Condensate Drain Connection Diameter##pipe_size##inches,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,Fan Drive##other##,Compressor Type##other##,Description##other##,Product Page URL##other##,Series##other##,Model##other##,Refrigerant Used##other##,Standards##other##,Base Rail Height##length##inches,Minimum Operation Clearance##length##inches,Service Clearance##length##inches,Front Side Service Clearance##length##inches,Downflow Return Duct Vertical Offset##length##inches,Downflow Supply Duct Vertical Offset##length##inches,Downflow Return Air Connection Height##hvac_duct_size##inches,Downflow Return Air Connection Width##hvac_duct_size##inches,Downflow Return Duct Horizontal Offset##length##inches,Downflow Supply Air Connection Height##hvac_duct_size##inches,Downflow Supply Air Connection Width##hvac_duct_size##inches,Downflow Supply Duct Horizontal Offset##length##inches,Drain Connection Horizontal Offset##length##inches,Drain Connection Vertical Offset##length##inches,Enclosure Depth##length##inches,Enclosure Width##length##inches,Horizontal Return Air Connection Height##hvac_duct_size##inches,Horizontal Return Air Connection Width##hvac_duct_size##inches,Horizontal Return Duct Horizontal Offset##length##inches,Horizontal Return Duct Vertical Offset##length##inches,Horizontal Supply Air Connection Height##hvac_duct_size##inches,Horizontal Supply Air Connection Width##hvac_duct_size##inches,Horizontal Supply Duct Horizontal Offset##length##inches,Horizontal Supply Duct Vertical Offset##length##inches,Outdoor Fan Diameter##length##inches
7.5Ton_230V_ZHD,87000,7.5,Two Speed,208 VAC - 230 VAC,240,11,14.1,5000,2000,1225,66,3,1,60.125,48.875,95.375,Belt Drive,Single-Stage & Two-Stage Scroll Compressor,Packaged Heat Pump Rooftop Unit,https://www.allied-commercial.com/products/packaged-rooftop-units/,Z-Series,ZHD,R-454B,ASHRAE 90.1 Compliant,3.5,36,36,60,10.5,10.5,39,14.5,39.375,15,28.25,5,37.75,6.875,58.125,93.375,38.75,14.625,42.625,6,14.5,30.25,3.375,6,24
8.5Ton_230V_ZHD,100000,8.5,Two Speed,208 VAC - 230 VAC,240,11,14.1,5000,2000,1225,66,3,1,60.125,48.875,95.375,Belt Drive,Single-Stage & Two-Stage Scroll Compressor,Packaged Heat Pump Rooftop Unit,https://www.allied-commercial.com/products/packaged-rooftop-units/,Z-Series,ZHD,R-454B,ASHRAE 90.1 Compliant,3.5,36,36,60,10.5,10.5,39,14.5,39.375,15,28.25,5,37.75,6.875,58.125,93.375,38.75,14.625,42.625,6,14.5,30.25,3.375,6,24
10Ton_230V_ZHD,118000,10,MSAV® (Multi-Stage Air Volume),208 VAC - 230 VAC,240,11,14.1,6250,2000,1290,66,3,1,60.125,48.875,95.375,Belt Drive,Single-Stage & Two-Stage Scroll Compressor,Packaged Heat Pump Rooftop Unit,https://www.allied-commercial.com/products/packaged-rooftop-units/,Z-Series,ZHD,R-454B,ASHRAE 90.1 Compliant,3.5,36,36,60,10.5,10.5,39,14.5,39.375,15,28.25,5,37.75,6.875,58.125,93.375,38.75,14.625,42.625,6,14.5,30.25,3.375,6,24
7.5Ton_460V_ZHD,87000,7.5,Two Speed,460 VAC,480,11,14.1,5000,2000,1225,66,3,1,60.125,48.875,95.375,Belt Drive,Single-Stage & Two-Stage Scroll Compressor,Packaged Heat Pump Rooftop Unit,https://www.allied-commercial.com/products/packaged-rooftop-units/,Z-Series,ZHD,R-454B,ASHRAE 90.1 Compliant,3.5,36,36,60,10.5,10.5,39,14.5,39.375,15,28.25,5,37.75,6.875,58.125,93.375,38.75,14.625,42.625,6,14.5,30.25,3.375,6,24
8.5Ton_460V_ZHD,100000,8.5,Two Speed,460 VAC,480,11,14.1,5000,2000,1225,66,3,1,60.125,48.875,95.375,Belt Drive,Single-Stage & Two-Stage Scroll Compressor,Packaged Heat Pump Rooftop Unit,https://www.allied-commercial.com/products/packaged-rooftop-units/,Z-Series,ZHD,R-454B,ASHRAE 90.1 Compliant,3.5,36,36,60,10.5,10.5,39,14.5,39.375,15,28.25,5,37.75,6.875,58.125,93.375,38.75,14.625,42.625,6,14.5,30.25,3.375,6,24
10Ton_460V_ZHD,118000,10,MSAV® (Multi-Stage Air Volume),460 VAC,480,11,14.1,6250,2000,1290,66,3,1,60.125,48.875,95.375,Belt Drive,Single-Stage & Two-Stage Scroll Compressor,Packaged Heat Pump Rooftop Unit,https://www.allied-commercial.com/products/packaged-rooftop-units/,Z-Series,ZHD,R-454B,ASHRAE 90.1 Compliant,3.5,36,36,60,10.5,10.5,39,14.5,39.375,15,28.25,5,37.75,6.875,58.125,93.375,38.75,14.625,42.625,6,14.5,30.25,3.375,6,24
7.5Ton_575V_ZHD,87000,7.5,Two Speed,575 VAC,600,11,14.1,5000,2000,1225,66,3,1,60.125,48.875,95.375,Belt Drive,Single-Stage & Two-Stage Scroll Compressor,Packaged Heat Pump Rooftop Unit,https://www.allied-commercial.com/products/packaged-rooftop-units/,Z-Series,ZHD,R-454B,ASHRAE 90.1 Compliant,3.5,36,36,60,10.5,10.5,39,14.5,39.375,15,28.25,5,37.75,6.875,58.125,93.375,38.75,14.625,42.625,6,14.5,30.25,3.375,6,24
8.5Ton_575V_ZHD,100000,8.5,Two Speed,575 VAC,600,11,14.1,5000,2000,1225,66,3,1,60.125,48.875,95.375,Belt Drive,Single-Stage & Two-Stage Scroll Compressor,Packaged Heat Pump Rooftop Unit,https://www.allied-commercial.com/products/packaged-rooftop-units/,Z-Series,ZHD,R-454B,ASHRAE 90.1 Compliant,3.5,36,36,60,10.5,10.5,39,14.5,39.375,15,28.25,5,37.75,6.875,58.125,93.375,38.75,14.625,42.625,6,14.5,30.25,3.375,6,24
10Ton_575V_ZHD,118000,10,MSAV® (Multi-Stage Air Volume),575 VAC,600,11,14.1,6250,2000,1290,66,3,1,60.125,48.875,95.375,Belt Drive,Single-Stage & Two-Stage Scroll Compressor,Packaged Heat Pump Rooftop Unit,https://www.allied-commercial.com/products/packaged-rooftop-units/,Z-Series,ZHD,R-454B,ASHRAE 90.1 Compliant,3.5,36,36,60,10.5,10.5,39,14.5,39.375,15,28.25,5,37.75,6.875,58.125,93.375,38.75,14.625,42.625,6,14.5,30.25,3.375,6,24
